I purchased this gun used about 1 month ago. I have fire approximately 150 rounds in 3 separate sessions at a range. I have had a Failure to Extract/Eject on nearly EVERY magazine. The ammo used was Magtech FMJ, Remmington FMJ, and Monarch JHP. Just to make sure that I wasn’t “limp wristing” I had the manager at the range also fired the gun. In 2, 6 round magazines he had the same issue twice. The FTE problem is on any round in the magazine, 1 thru 6, and regardless of the number of rounds in the magazine, 3 to 6 rounds in the magazine. The gun was cleaned and oiled after each session.

Please repair or replace at your earliest convenience.

Thanks,

Gene Maurice